**INPUT FROM CC AND OCS PROCESS AND STORED DATA IN MEMORY**

**If message status is received**

NO

**LED WILL BE ON**

YES

**LED WILL BLINK CONTIONUSLY 1 SEC**

**RESET**

**EEPROM**

**FLOW CHART OF INSTRUMENT CLUSTER**