**CC**

CC warning lamp status given to the IC ECU.

**ECU**

**OCS ECU**

Airbag warning lamp status given to the IC ECU

READ CAN

SYS\_INIT

CAN\_INIT

SET\_BAUDRATE

SET\_MASK

SET\_FILTER

CAN\_READ

**Instrument cluster ECU**

Received input status process and stored in EEPROM.

After storing status checking condition for the receiving input status is valid or invalid.

Using this switch clear all the received data in memory.

**Trip Switch Reset**

If input status is valid then warning lamp blink continuously with delay 1sec else warning lamp should be in ON state

**FUNCTIONAL BLOCK DIAGRAM**